#

##

##

    礦ision Build Log
    Project:
    E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\ST7775 STM32 IO 8b\ST7775 STM32 IO 8b\USER\LCD.uvproj
    Project File Date:  05/07/2014

    Output:
    Build target 'Target 1'
    compiling main.c...
    main.c(11): warning:  #177-D: variable "x" was declared but never referenced
            u8 x=0;
    main.c: 1 warning, 0 errors
    linking...
    Program Size: Code=9166 RO-data=77738 RW-data=60 ZI-data=1092
    FromELF: creating hex file...
    ".\LCD.axf" - 0 Error(s), 1 Warning(s).
    Load "E:\\Sync_WangXinYue\\LCD-200\\最终资料\\ArduinoSTM32\\ST7775 STM32 IO 8b\\ST7775 STM32 IO 8b\\USER\\LCD.axf"
    Set JLink Project File to "E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\ST7775 STM32 IO 8b\ST7775 STM32 IO 8b\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103VB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM V8 compiled Jul 17 2013 11:24:15
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103VB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...