#

##

##

    µVision Build Log
    Project:
    F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\LCD.uvproj
    Project File Date:  03/20/2014

    Output:
    Build target 'Target 1'
    linking...
    Program Size: Code=12504 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    linking...
    Program Size: Code=12504 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    linking...
    Program Size: Code=12504 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: STM32F1xxx: Can not attach to CPU. Trying connect under reset.
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling main.c...
    main.c(24): warning:  #940-D: missing return statement at end of non-void function "IO_Check"
    linking...
    Program Size: Code=12156 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 1 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    linking...
    Program Size: Code=12156 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12204 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    compiling lcd.c...
    "..\HARDWARE\LCD\lcd.c" - 0 Errors, 0 Warning(s).
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12220 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: STM32F1xxx: Can not attach to CPU. Trying connect under reset.
    Rebuild target 'Target 1'
    compiling main.c...
    main.c(24): warning:  #940-D: missing return statement at end of non-void function "IO_Check"
    compiling stm32f10x_it.c...
    compiling system_stm32f10x.c...
    compiling led.c...
    compiling key.c...
    compiling exti.c...
    compiling wdg.c...
    compiling timer.c...
    compiling pwm.c...
    compiling lcd.c...
    compiling delay.c...
    compiling sys.c...
    compiling usart.c...
    compiling core_cm3.c...
    assembling startup_stm32f10x_md.s...
    compiling misc.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_cec.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    linking...
    Program Size: Code=12220 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 1 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    ***JLink Error: Can not read register 0 (R0) while CPU is running
    ***JLink Error: Can not read register 1 (R1) while CPU is running
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12208 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    linking...
    Program Size: Code=12208 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12220 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12220 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    compiling lcd.c...
    "..\HARDWARE\LCD\lcd.c" - 0 Errors, 0 Warning(s).
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12220 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12236 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12208 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Build target 'Target 1'
    compiling main.c...
    main.c(24): warning:  #940-D: missing return statement at end of non-void function "IO_Check"
    linking...
    Program Size: Code=12204 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 1 Warning(s).
    Build target 'Target 1'
    compiling main.c...
    main.c(24): warning:  #940-D: missing return statement at end of non-void function "IO_Check"
    linking...
    Program Size: Code=12144 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 1 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12128 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Build target 'Target 1'
    linking...
    Program Size: Code=12128 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Build target 'Target 1'
    linking...
    Program Size: Code=12128 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling main.c...
    main.c(24): warning:  #940-D: missing return statement at end of non-void function "IO_Check"
    linking...
    Program Size: Code=12156 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 1 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling main.c...
    main.c(24): warning:  #940-D: missing return statement at end of non-void function "IO_Check"
    linking...
    Program Size: Code=12188 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 1 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=12204 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "F:\\IH_LuoPinChao\\Projects\\2.0inch TFT LCD\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "F:\IH_LuoPinChao\Projects\2.0inch TFT LCD\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...