#

##

##

    礦ision Build Log
    Project:
    C:\Documents and Settings\Administrator\桌面\0164 nt3916  16B\USER\LCD.uvproj
    Project File Date:  03/27/2014

    Output:
    Load "C:\\Documents and Settings\\Administrator\\桌面\\0164 nt3916  16B\\USER\\LCD.axf"
    Set JLink Project File to "C:\Documents and Settings\Administrator\桌面\0164 nt3916  16B\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.313V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 0
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'Target 1'
    linking...
    Program Size: Code=14788 RO-data=2968 RW-data=60 ZI-data=1700
    FromELF: creating hex file...
    ".\LCD.axf" - 0 Errors, 0 Warning(s).
    Load "C:\\Documents and Settings\\Administrator\\桌面\\0164 nt3916  16B\\USER\\LCD.axf"
    Set JLink Project File to "C:\Documents and Settings\Administrator\桌面\0164 nt3916  16B\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.68a, compiled Apr 12 2013 13:26:50
    Firmware: J-Link ARM V8 compiled Nov 14 2012 22:34:52
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.306V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...