#

##

##

    礦ision Build Log
    Project:
    E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\LCD.uvproj
    Project File Date:  05/07/2014

    Output:
    Build target 'Target 1'
    linking...
    Program Size: Code=13640 RO-data=2968 RW-data=60 ZI-data=1700
    ".\LCD.axf" - 0 Error(s), 0 Warning(s).
    Load "E:\\Sync_WangXinYue\\LCD-200\\最终资料\\ArduinoSTM32\\ILI9225 STM32 16B IO\\ILI9225 STM32 16B IO\\USER\\LCD.axf"
    Set JLink Project File to "E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\ILI9225 STM32 16B IO\ILI9225 STM32 16B IO\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103VB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM V8 compiled Jul 17 2013 11:24:15
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103VB
    VTarget = 3.325V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...

_spi.c... compiling stm32f10x_tim.c... compiling stm32f10x_usart.c... compiling stm32f10x_wwdg.c... compiling gui.c... linking... .\LCD.axf: Error: L6218E: Undefined symbol delay (referred from main.o). Not enough information to list image symbols. Finished: 1 information, 0 warning and 1 error messages. ".\LCD.axf" - 1 Error(s), 3 Warning(s). Target not created compiling main.c... main.c(25): warning: #940-D: missing return statement at end of non-void function "IO_Check" } main.c(42): warning: #223-D: function "delay_" declared implicitly delay_(100); main.c(29): warning: #177-D: variable "x" was declared but never referenced u8 x=0; main.c: 3 warnings, 0 errors "main.c" - 0 Error(s), 3 Warning(s). compiling main.c... main.c(25): warning: #940-D: missing return statement at end of non-void function "IO_Check" } main.c(29): warning: #177-D: variable "x" was declared but never referenced u8 x=0; main.c: 2 warnings, 0 errors "main.c" - 0 Error(s), 2 Warning(s). TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 4000 kHz Erase Done. Programming Done. Verify OK. Application running ... compiling main.c... main.c(25): warning: #940-D: missing return statement at end of non-void function "IO_Check" } main.c(40): warning: #223-D: function "delay" declared implicitly delay(100); main.c(29): warning: #177-D: variable "x" was declared but never referenced u8 x=0; main.c: 3 warnings, 0 errors "main.c" - 0 Error(s), 3 Warning(s).