#

##

##

    礦ision Build Log
    Project:
    E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\0164 nt3916  16B 39pin\USER\LCD.uvproj
    Project File Date:  05/07/2014

    Output:
    Rebuild target 'Target 1'
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling system_stm32f10x.c...
    compiling led.c...
    compiling key.c...
    compiling exti.c...
    compiling wdg.c...
    compiling timer.c...
    compiling pwm.c...
    compiling lcd.c...
    compiling delay.c...
    compiling sys.c...
    compiling usart.c...
    compiling core_cm3.c...
    assembling startup_stm32f10x_md.s...
    compiling misc.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_cec.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    linking...
    Program Size: Code=11948 RO-data=2928 RW-data=60 ZI-data=1700
    FromELF: creating hex file...
    ".\LCD.axf" - 0 Error(s), 0 Warning(s).
    Load "E:\\Sync_WangXinYue\\LCD-200\\最终资料\\ArduinoSTM32\\0164 nt3916  16B 39pin\\USER\\LCD.axf"
    Set JLink Project File to "E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\0164 nt3916  16B 39pin\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103VB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM V8 compiled Jul 17 2013 11:24:15
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: STM32F1xxx: Can not attach to CPU. Trying connect under reset.
    **JLink Warning: RESET (pin 15) high, but should be low. Please check target hardware.
    ***JLink Error: Supply voltage too low (1 Volt is required, Measured: 0.0 Volt).
    Please check target power.
    Error: Flash Download failed  -  Target DLL has been cancelled
    Load "E:\\Sync_WangXinYue\\LCD-200\\最终资料\\ArduinoSTM32\\0164 nt3916  16B 39pin\\USER\\LCD.axf"
    Set JLink Project File to "E:\Sync_WangXinYue\LCD-200\最终资料\ArduinoSTM32\0164 nt3916  16B 39pin\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103VB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM V8 compiled Jul 17 2013 11:24:15
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103VB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...