//==============================================================
// Inhaos 2017/05/22
//
// Ardunio 3rd-party hardware package for MD8F
//	Installation Guide
// 
// Update memo:
// v3.6
//	- update mainly for MD328P support 
//	- add VUSB support library
// v4.6
//	- add MD3248P support (development board name UNP Pro)
//
//==============================================================

1. Features
	> Support arduino 1.0.x/1.5.x/1.6.x
	> Support bootloader by optiboot
	> Bootloader baudrate: 115200bps
	> Support board: Massduino & MD88A MiniDev
	> Support board: Massduino w/ MD8FX8D and MD3248P

2. Package contents
	Massduino_HSP_v4.6 : package root directory
	|
	+ hardware : 3rd party hardware support package
	|    |
	|    + MD : package for support arduino 1.5.x/1.6.x
	|    |
	|    + MD8F : package for support arduino 1.0.x
	|
	+ libraries : 3rd party hardware library

3. Installation:
	> Unzip Massduino_HSP_v4.5.rar
	> Copy [sketches], [hardware] and [libraries] directories to arduino's sketchbook direcotry
	> Restart Arduino, you will see new board from [Tools]->[Border] menu.

4. about arduino's sketchbook directory:
	You can always find this directory from [File]->[Preferences] menu.
	Here is the default sketchbook directory for most popluar system:
	> Windows: C:\Users\<Username>\Documents\Arduino
	> Mac OSX: /Users/user/Documents/Arduino
	> LINUX: /home/<Username>/sketchbook
